List of global parameters:
AUTO_UPDATE_OPTIONS = 
CFGSERV_APP_NAME = DBProvider
CFGSERV_BINDING_INTERFACE = 127.0.0.1
CFGSERV_BINDING_PORT = 5485
DB_VERSION = 346
INST_ALLOW_MODIFY = 1
INST_AUTODELETE_RECORDINGS = 0
INST_AUTODELETE_VOICEMAIL = 0
INST_BACKUP_REPOSITORY = /var/lib/3cxpbx/Instance1/Data/Backups
INST_BACKUP_REPOSITORY_PASS = *****
INST_BACKUP_REPOSITORY_USER = 
INST_CALLUS_LINK_EXT = http://scrfhc.east.3cx.us:5000/webrtc
INST_CALLUS_LINK_EXT_SEC = https://scrfhc.east.3cx.us:5001/webrtc
INST_CALLUS_LINK_LOCAL = http://192.168.23.250:5000/webrtc
INST_CALLUS_LINK_LOCAL_SEC = https://192.168.23.250:5001/webrtc
INST_CHR_CONN_IP = 127.0.0.1
INST_CHR_CONN_PORT = 5484
INST_CHR_LISTEN_IP = 127.0.0.1
INST_CHR_LISTEN_PORT = 5484
INST_CLOUD_ADMIN_EMAIL = 
INST_CLOUD_WEB_SERVICE = http://localhost:5000/3CXCloudWebService
INST_CM_API_INTERFACE = 127.0.0.1
INST_CM_API_IP = 127.0.0.1
INST_CM_API_PASSWORD = *****
INST_CM_API_PORT = 5482
INST_CM_API_USER = instance_Instance142757
INST_DATADIR = /var/lib/3cxpbx/Instance1
INST_DEFAULT_CONFIGURED_PUBLIC_IP = 64.223.141.38
INST_ERPEXTERNALFQDN = scrfhc
INST_ERPFQDNCODE = east-us
INST_ERPINTERNALFQDN = 192.168.23.250
INST_FAILOVER_OPTIONS = 
INST_INITIAL_CONFGATEWAY = 
INST_INITIAL_ENL = 
INST_INITIAL_FAXOVEREMAILGATEWAY = 
INST_INITIAL_LANGUAGE = 
INST_INITIAL_MLFROMADDR = 
INST_INITIAL_MLSRVADDR = 
INST_INITIAL_MLSRVPASSWORD = *****
INST_INITIAL_MLSRVPORT = 
INST_INITIAL_MLSRVTLS = 
INST_INITIAL_MLSRVUSER = 
INST_INITIAL_NOTALLOWED_COUNTRYCODES = 
INST_INITIAL_PINPROTECTIVR = 
INST_INITIAL_PROVISIONING_FOLDER = 
INST_INITIAL_VOICEMAIL_SPECIALMENU = 
INST_INITIAL_WEBSERVERPASS = *****
INST_INITIAL_WEBSERVERUSER = 
INST_IVR_RTPFIRST = 12000
INST_IVR_RTPLAST = 13999
INST_IVR_SIPINTERFACE = 127.0.0.1
INST_IVR_SIPPORT = 5483
INST_LICENSEKEY = 3Y7M-I9MQ-RIWB-GD60
INST_MAILFROMADDRESS = emailvoicemails@gmail.com
INST_MAILSERVERHOST = smtp.gmail.com
INST_MAILSERVERPASS = *****
INST_MAILSERVERPORT = 587
INST_MAILSERVERUSER = emailvoicemails@gmail.com
INST_MAILSERVERUSETLS = True
INST_MANAGEMENT_LINK_EXT = http://scrfhc.east.3cx.us:5000/management
INST_MANAGEMENT_LINK_EXT_SEC = https://scrfhc.east.3cx.us:5001/management
INST_MANAGEMENT_LINK_LOCAL = http://192.168.23.250:5000/management
INST_MANAGEMENT_LINK_LOCAL_SEC = https://192.168.23.250:5001/management
INST_MYPHONE_LINK_EXT = http://scrfhc.east.3cx.us:5000/myphone/MPWebService.asmx
INST_MYPHONE_LINK_EXT_SEC = https://scrfhc.east.3cx.us:5001/myphone/MPWebService.asmx
INST_MYPHONE_LINK_LOCAL = http://192.168.23.250:5000/myphone/MPWebService.asmx
INST_MYPHONE_LINK_LOCAL_SEC = https://192.168.23.250:5001/myphone/MPWebService.asmx
INST_NETWORKINSTALLATION = NAT
INST_NGINXCERTFOLDER = /var/lib/3cxpbx/Bin/nginx/conf/Instance1
INST_NOTIFY_SERVICES_DOWN = 1
INST_PBXPUBLICIP = scrfhc.east.3cx.us
INST_PROMPT_PATH = /var/lib/3cxpbx/Instance1/Data/Ivr/Prompts
INST_PROMPT_WEBACCESS_URL = /var/lib/3cxpbx/Instance1/Data/Ivr/Prompts
INST_PROVISIONING_FOLDER = *****
INST_PROVISIONING_FOLDER_ROOT = /var/lib/3cxpbx/Instance1/Data/Http/Interface/provisioning
INST_PROVISIONING_LINK_EXT = http://scrfhc.east.3cx.us:5000/provisioning
INST_PROVISIONING_LINK_EXT_SEC = https://scrfhc.east.3cx.us:5001/provisioning
INST_PROVISIONING_LINK_LOCAL = http://192.168.23.250:5000/provisioning
INST_PROVISIONING_LINK_LOCAL_SEC = https://192.168.23.250:5001/provisioning
INST_QUOTA_RECORDINGS = 5
INST_QUOTA_VMBOX = 5
INST_RECORDING_PATH = /var/lib/3cxpbx/Instance1/Data/Recordings
INST_RECORDING_WEBACCESS_URL = /var/lib/3cxpbx/Instance1/Data/Recordings
INST_REPORTER_LINK_EXT = http://scrfhc.east.3cx.us:5000/Reporter
INST_REPORTER_LINK_EXT_SEC = https://scrfhc.east.3cx.us:5001/Reporter
INST_REPORTER_LINK_LOCAL = http://192.168.23.250:5000/Reporter
INST_REPORTER_LINK_LOCAL_SEC = https://192.168.23.250:5001/Reporter
INST_SIPDOMAIN = scrfhc.east.3cx.us
INST_SIPDOMAIN_LOCAL = 192.168.23.250
INST_SIPEXTERNALIP = 64.223.141.38
INST_SIPLOCALIP = 192.168.23.250
INST_SIPPORT = 5060
INST_STUNDISABLED = 1
INST_TNL_CLIENT_LISTEN_INTERFACE = 
INST_TNL_CLIENT_LISTEN_PORT = 5090
INST_TNL_CLIENT_SIPINTERFACE = 127.0.0.1
INST_TNL_CLIENT_SIPPORT = 5080
INST_TNL_RTPFIRST = 14000
INST_TNL_RTPLAST = 14999
INST_USE3CXFQDN = 1
INST_USER_CFGSERVER_PASSWORD = *****
INST_USER_CFGSERVER_USER = cfguser_default
INST_VOICEMAILBOX_PATH = /var/lib/3cxpbx/Instance1/Data/Ivr/Voicemail
INST_VOICEMAILBOX_WEBACCESS_URL = /var/lib/3cxpbx/Instance1/Data/Ivr/Voicemail
INST_WEB_ROOT_EXT = http://scrfhc.east.3cx.us:5000/
INST_WEB_ROOT_EXT_SEC = https://scrfhc.east.3cx.us:5001/
INST_WEB_ROOT_LOCAL = http://192.168.23.250:5000/
INST_WEB_ROOT_LOCAL_SEC = https://192.168.23.250:5001/
INST_WEBMEETING_FQDN = scrfhc-east-us.3cx.net
INST_WEBRTC_GATEWAY_IP = 127.0.0.1
INST_WRTC_EXTERNALADDRESS = 64.223.141.38
INST_WRTC_INTERFACE = 192.168.23.250
INST_WRTC_MEDIAFIRST = 9256
INST_WRTC_MEDIALAST = 9499
INST_WRTC_RTPFIRST = 7500
INST_WRTC_RTPLAST = 7755
INST_WRTC_SIPPORT = 5062
MAIL_SERVER_TYPE = 3CX
UPDATE_LINK = 
